# Template file for 'rpi-kernel'
#
# Latest commit as of 20140226
_githash="4f27bd0d364ba6cb15a924c072300c18f28d7572"
_gitshort="${_githash:0:7}"

pkgname=rpi-kernel
version=3.10.32
revision=1
wrksrc="linux-${_githash}"
maintainer="Juan RP <xtraeme@gmail.com>"
homepage="http://www.kernel.org"
license="GPL-2"
short_desc="The Linux kernel and modules for the Raspberry Pi (${version%.*} series [git ${_gitshort}])"
distfiles="https://github.com/raspberrypi/linux/archive/${_githash}.tar.gz"
checksum=366f615786f8fabf5bf25d3622da8057b6b3358798a5a2f0831c0bdad4909544

_kernver="${version}_${revision}"

create_srcdir=yes
nostrip=yes
noverifyrdeps=yes

only_for_archs="armv6l"
hostmakedepends="perl python kmod>=11_2 uboot-mkimage openssl which elfutils bc"
makedepends="ncurses-devel"
depends="kmod>=11_2"
replaces="kernel-rpi>=0"
triggers="kernel-hooks"
# These files could be modified when an external module is built.
mutable_files="
	/usr/lib/modules/${_kernver}/modules.dep
	/usr/lib/modules/${_kernver}/modules.dep.bin
	/usr/lib/modules/${_kernver}/modules.symbols
	/usr/lib/modules/${_kernver}/modules.symbols.bin
	/usr/lib/modules/${_kernver}/modules.alias
	/usr/lib/modules/${_kernver}/modules.alias.bin
	/usr/lib/modules/${_kernver}/modules.devname"

pre_configure() {
	# Remove .git directory, otherwise scripts/setkernelversion.sh
	# modifies KERNELRELEASE and appends + to it.
	rm -rf .git
}

do_configure() {
	if [ "$CROSS_BUILD" ]; then
		_args="CROSS_COMPILE=${XBPS_CROSS_TRIPLET}-"
	fi

	# Copy required files to create the bootable image.
	cp ${FILESDIR}/args-uncompressed.txt arch/arm/boot/
	cp ${FILESDIR}/boot-uncompressed.txt arch/arm/boot/
	cp ${FILESDIR}/imagetool-uncompressed.py arch/arm/boot/

	# Use upstream default configuration, no need to maintain ours.
	make ${makejobs} ${_args} ARCH=arm bcmrpi_defconfig

	# Always use our revision to CONFIG_LOCALVERSION to match our pkg version.
	sed -i -e "s|^\(CONFIG_LOCALVERSION=\).*|\1\"_${revision}\"|" .config
}

do_build() {
	if [ "$CROSS_BUILD" ]; then
		_args="CROSS_COMPILE=${XBPS_CROSS_TRIPLET}-"
	fi
	make ${makejobs} ${_args} ARCH=arm prepare
	make ${makejobs} ${_args} ARCH=arm uImage modules
}

do_install() {
	local hdrdest

	# Run depmod after compressing modules.
	sed -i '2iexit 0' scripts/depmod.sh

	# Install kernel, firmware and modules
	make ARCH=arm INSTALL_MOD_PATH=${DESTDIR} modules_install

	# Generate kernel.img and install it to destdir.
	cd arch/arm/boot
	/usr/bin/python2 imagetool-uncompressed.py
	cd ${wrksrc}
	vinstall arch/arm/boot/kernel.img 644 boot

	hdrdest=${DESTDIR}/usr/src/${sourcepkg}-headers-${_kernver}

	# Switch to /usr.
	vmkdir usr
	mv ${DESTDIR}/lib ${DESTDIR}/usr

	cd ${DESTDIR}/usr/lib/modules/${_kernver}
	rm -f source build
	ln -sf ../../../src/${sourcepkg}-headers-${_kernver} build

	cd ${wrksrc}
	# Install required headers to build external modules
	install -Dm644 Makefile ${hdrdest}/Makefile
	install -Dm644 kernel/Makefile ${hdrdest}/kernel/Makefile
	install -Dm644 .config ${hdrdest}/.config
	mkdir -p ${hdrdest}/include

	# Remove firmware stuff provided by the "linux-firmware" pkg.
	rm -rf ${DESTDIR}/usr/lib/firmware

	for i in acpi asm-generic config crypto drm generated linux math-emu \
		media net pcmcia scsi sound trace video xen; do
		[ -d include/$i ] && cp -a include/$i ${hdrdest}/include
	done

	cd ${wrksrc}
	# Copy files necessary for later builds.
	cp Module.symvers ${hdrdest}
	cp -a scripts ${hdrdest}

	# fix permissions on scripts dir
	chmod og-w -R ${hdrdest}/scripts

	# copy arch includes for external modules
	mkdir -p ${hdrdest}/arch/arm/mach-bcm2708
	cp -a arch/arm/include ${hdrdest}/arch/arm
	cp -a arch/arm/mach-bcm2708/include ${hdrdest}/arch/arm/mach-bcm2708

	mkdir -p ${hdrdest}/arch/arm/kernel

	cp arch/arm/Makefile ${hdrdest}/arch/arm
	cp arch/arm/kernel/asm-offsets.s ${hdrdest}/arch/arm/kernel

	# Add docbook makefile
	install -Dm644 Documentation/DocBook/Makefile \
		${hdrdest}/Documentation/DocBook/Makefile

	# Add md headers
	mkdir -p ${hdrdest}/drivers/md
	cp drivers/md/*.h ${hdrdest}/drivers/md

	# Add inotify.h
	mkdir -p ${hdrdest}/include/linux
	cp include/linux/inotify.h ${hdrdest}/include/linux

	# Add wireless headers
	mkdir -p ${hdrdest}/net/mac80211/
	cp net/mac80211/*.h ${hdrdest}/net/mac80211

	# add dvb headers for external modules
	mkdir -p ${hdrdest}/include/config/dvb/
	cp include/config/dvb/*.h ${hdrdest}/include/config/dvb/

	# Copy in Kconfig files
	for i in $(find . -name "Kconfig*"); do
		mkdir -p ${hdrdest}/$(echo $i | sed 's|/Kconfig.*||')
		cp $i ${hdrdest}/$i
	done

	# Remove unneeded architectures
	for arch in alpha arm26 avr32 blackfin cris frv h8300 \
		ia64 m* p* s* um v850 x86 xtensa; do
		rm -rf ${hdrdest}/arch/${arch}
	done

	# Compress all modules with xz to save a few MBs.
	msg_normal "$pkgver: compressing kernel modules with gzip, please wait...\n"
	find ${DESTDIR} -name '*.ko' -exec gzip -9 {} \;

	# ... and run depmod again.
	depmod -b ${DESTDIR}/usr -F System.map ${_kernver}
}

rpi-kernel-headers_package() {
	nostrip=yes
	noverifyrdeps=yes
	replaces="kernel-rpi-headers>=0"
	short_desc="The Linux kernel headers for the Raspberry Pi (${version%.*} series [git ${_gitshort}])"
	pkg_install() {
		vmove usr/src
		vmove usr/lib/modules/${_kernver}/build
	}
}
