Firmware is now compressed with zstd. Ensure you are running a supported kernel:

- linux5.10>=5.10.251_1
- linux5.15>=5.15.201_1
- linux6.1>=6.1.127_1
- linux6.6>=6.6.68_1
- linux6.12>=6.12.7_1
- linux6.18, linux6.19, or any later version
- rpi-kernel>=6.12.67_1
- pinephone-kernel>=6.1.7_2

For more information, read: https://voidlinux.org/news/2026/03/firmware-compression.html
