put vtv_end.o in front of postdep_objects_CXX
having it after crtendS.o leads to missing zero termination in eh_frame section

This is in line with comment in libgcc/vtv_end.c:

   When the GCC driver inserts vtv_start.o into the link line (just
   after crtbegin.o) it also inserts vtv_end.o into the link line,
   just before crtend.o.

--- a/libstdc++-v3/configure
+++ b/libstdc++-v3/configure
@@ -15762,7 +15762,7 @@ fi
 
 if test "$enable_vtable_verify" = yes; then
   predep_objects_CXX="${predep_objects_CXX} ${glibcxx_builddir}/../libgcc/vtv_start.o"
-  postdep_objects_CXX="${postdep_objects_CXX} ${glibcxx_builddir}/../libgcc/vtv_end.o"
+  postdep_objects_CXX="${glibcxx_builddir}/../libgcc/vtv_end.o ${postdep_objects_CXX}" 
 fi
 
 
