--- a/src/wl/sys/wl_cfg80211_hybrid.c
+++ b/src/wl/sys/wl_cfg80211_hybrid.c
@@ -30,6 +30,9 @@
 #include <linux/kthread.h>
 #include <linux/netdevice.h>
 #include <linux/ieee80211.h>
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 11, 0)
+	#include <linux/sched/signal.h>
+#endif
 #include <net/cfg80211.h>
 #include <linux/nl80211.h>
 #include <net/rtnetlink.h>
--- a/src/wl/sys/wl_linux.c
+++ b/src/wl/sys/wl_linux.c
@@ -117,6 +117,9 @@ int wl_found = 0;
 
 typedef struct priv_link {
 	wl_if_t *wlif;
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 11, 0)
+	unsigned long last_rx;
+#endif
 } priv_link_t;
 
 #define WL_DEV_IF(dev)          ((wl_if_t*)((priv_link_t*)DEV_PRIV(dev))->wlif)
@@ -2449,6 +2452,9 @@ wl_monitor(wl_info_t *wl, wl_rxsts_t *rx
 {
 	struct sk_buff *oskb = (struct sk_buff *)p;
 	struct sk_buff *skb;
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 11, 0)
+	priv_link_t *priv_link;
+#endif
 	uchar *pdata;
 	uint len;
 
@@ -2915,7 +2921,13 @@ wl_monitor(wl_info_t *wl, wl_rxsts_t *rx
 	if (skb == NULL) return;
 
 	skb->dev = wl->monitor_dev;
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 11, 0)
+	priv_link = MALLOC(wl->osh, sizeof(priv_link_t));
+	priv_link = netdev_priv(skb->dev);
+	priv_link->last_rx = jiffies;
+#else
 	skb->dev->last_rx = jiffies;
+#endif
 #if LINUX_VERSION_CODE >= KERNEL_VERSION(2, 6, 22)
 	skb_reset_mac_header(skb);
 #else
